Trail Access Information Summary	
Park Name	Piscassic Greenway	
Trail Name	Neal Mill Road	
Segment	Neal Mill Road	
Type			
Length	0.4 mi (0.7 km)		
Elevation Gain	40.5 ft (12.36 m)		
Elevation Loss	24.2 ft (7.37 m)		
Trail Uses Allowed			

Trail Uses NOT Allowed			

Typical Grade	2.8%	Max = 14.2%	
Intermediate			
Maximum			
	Standard Ramp Grade is 8.3%		
Typical Cross Slope	2.4%	Max = 9.3%	
Intermediate			
Maximum			
Typical Tread Width	24 in (61.0 cm)	Min = 24 in (61.0 cm)	
Intermediate			
Minimum			
Surface Type	Aggregate/ Gravel		
Surface Category	0.0 % of Trail is Paved	0.0 % of trail is Soft	
	100.0 % of Trail is Hard	0.0 % of trail is Very Soft	
	0.0 % of Trail is Firm		
Firmness	Typical: n/a	Minimum: n/a	
Stability	Typical: n/a	Minimum: n/a	
Obstructions:			
Type:	Size (Height):	Remaining Tread:	Location:	
n/a	n/a in (n/a cm)	n/a in (n/a cm)	n/a ft (n/a m)	
n/a	n/a in (n/a cm)	n/a in (n/a cm)	n/a (n/a m)	
n/a	n/a in (n/a cm)	n/a in (n/a cm)	n/a ft (n/a m)	
Warning: Trail conditions may have changed since  when this trail was assessed. Temporary obstacles were not mapped.	
Maximum grades and cross-slopes may vary. Obstructions less than ??? in (??? cm) or outside of the tread area 36 in (91.4 cm) wide by ??? in (??? cm) high were not reported. Minimum clearance width boundaries were at least ??? in (??? cm) high	
Signage created by Beneficial Designs Inc. from data collected by a Certified Trail Assessment Coordinator using the High Efficiency Trail Assessment Process (HETAP).	
Funded by: