Trail Access Information Summary	
Park Name	Spruce Swamp	
Trail Name	Garrison Trail	
		
Type	Linear		
Length	0.9 mi (1.5 km)		
Elevation Gain	159.0 ft (48.5 m)		
Elevation Loss	144.1 ft (43.9 m)		
Trail Uses Allowed	Bicycling - Mountain	Snow - Snowshoeing	
	Hiking		
	Snow - Skiing, Cross Country		
Trail Uses NOT Allowed	Equestrian		
	Motor Vehicles		
	Motor Vehicles - Snowmobiling		
Typical Grade	6.4%	Max = 27.9%	
Intermediate			
Maximum			
	Standard Ramp Grade is 8.3%		
Typical Cross Slope	5.5%	Max = 34.0%	
Intermediate			
Maximum			
Typical Tread Width	18 in (46.3 cm)	Min = 18 in (45.7 cm)	
Intermediate			
Minimum			
Surface Type	Duff		
Surface Category	0.0 % of Trail is Paved	0.0 % of trail is Soft	
	1.4 % of Trail is Hard	0.0 % of trail is Very Soft	
	98.6 % of Trail is Firm		
Firmness	Typical: n/a	Minimum: n/a	
Stability	Typical: n/a	Minimum: n/a	
Obstructions:			
Type:	Size (Height):	Remaining Tread:	Location:	
n/a	n/a in (n/a cm)	n/a in (n/a cm)	n/a ft (n/a m)	
n/a	n/a in (n/a cm)	n/a in (n/a cm)	n/a (n/a m)	
n/a	n/a in (n/a cm)	n/a in (n/a cm)	n/a ft (n/a m)	
Warning: Trail conditions may have changed since 2025-08-28 when this trail was assessed. Temporary obstacles were not mapped.	
Maximum grades and cross-slopes may vary. Obstructions less than ??? in (??? cm) or outside of the tread area 36 in (91.4 cm) wide by 120 in (304.8 cm) high were not reported. Minimum clearance width boundaries were at least ??? in (??? cm) high	
Signage created by Beneficial Designs Inc. from data collected by a Certified Trail Assessment Coordinator using the High Efficiency Trail Assessment Process (HETAP).	
Funded by: